<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<library>
<description>MCP6401 general purpose op-amp</description>
<packages>
<package name="SOT-23-5">
</package>
</packages>
<symbols>
<symbol name="MCP6041">
<pin name="VIN-"/>
<pin name="VIN+"/>
<pin name="VSS"/>
<pin name="VOUT"/>
<pin name="VDD"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MCP6041" prefix="OP">
<description>&lt;b&gt;600 nA, Rail-to-Rail Input/Output Op Amps&lt;/b&gt;&lt;br&gt;
&lt;p&gt;
The MCP6041/2/3/4 family of operational amplifiers (op amps) from Microchip Technology Inc. operate with a single supply voltage as low as 1.4V, while drawing less than 1 μA (maximum) of quiescent current per amplifier. These devices are also designed to support rail-to-rail input and output operation. This combination of features supports battery-powered and portable applications.
The MCP6041/2/3/4 amplifiers have a gain-bandwidth product of 14 kHz (typical) and are unity gain stable. These specifications make these op amps appropriate for low frequency applications, such as battery current monitoring and sensor conditioning.&lt;/p&gt;
&lt;p&gt;The MCP6041/2/3/4 family operational amplifiers are offered in single (MCP6041), single with Chip Select (CS) (MCP6043), dual (MCP6042), and quad (MCP6044) configurations. The MCP6041 device is available in the 5-lead SOT-23 package, and the MCP6043 device is available in the 6-lead SOT-23 package.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MCP6041"/>
</gates>
<devices>
<device name="" package="SOT-23-5">
<connects>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VIN+" pad="3"/>
<connect gate="G$1" pin="VIN-" pad="4"/>
<connect gate="G$1" pin="VOUT" pad="1"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
