<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="-1" x2="22.5" y2="-1" width="0" layer="20"/>
<wire x1="22.5" y1="-1" x2="22.5" y2="17" width="0" layer="20"/>
<wire x1="22.5" y1="17" x2="0" y2="17" width="0" layer="20"/>
<wire x1="0" y1="17" x2="0" y2="-1" width="0" layer="20"/>
<text>MSP430 Breakout
Josiah Hester
Clemson University
</text>
<text>MSP430 Breakout
Josiah Hester
Clemson University
</text>
<text>GND</text>
<text>TEST</text>
<text>!RST</text>
<text>BATT+</text>
<text>BATT+</text>
<text>!RST</text>
<text>TEST</text>
<text>GND</text>
</plain>
<libraries>
<library name="msp430">
<packages>
<package name="PW_R-PDSO-G28">
<description>&lt;b&gt;PLASTIC SMALL-OUTLINE PACKAGE SO 28&lt;/b&gt; JEDEC MO-153, PW Type&lt;p&gt;
Source: www.ti.com/.. slvs087l.pdf</description>
</package>
</packages>
</library>
<library name="fc-135">
<packages>
<package name="FC-135_1PRIMARY">
<description>Original name &lt;b&gt;FC-135&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="ncp583">
<packages>
<package name="SC82-AB_1PRIMARY">
<description>Original name &lt;b&gt;SC82-AB&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="FKIT-LED-1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U2" library="msp430" package="PW_R-PDSO-G28" value="MSP430FR5728"/>
<element name="XTAL" library="fc-135" package="FC-135_1PRIMARY" value="FC-135"/>
<element name="U1" library="ncp583" package="SC82-AB_1PRIMARY" value="NCP583"/>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="100uF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="47kΩ">
<attribute name="PROD_ID" value="RES-08698"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="2.2nF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="2.2nF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="PRGM">
<attribute name="NAME"/>
</element>
<element name="LED1" library="SparkFun-LED" package="FKIT-LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="330Ω">
<attribute name="PROD_ID" value="RES-08698"/>
</element>
</elements>
<signals>
<signal name="BATT+">
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="26"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="25"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="!RST">
<contactref element="R1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U2" pad="18"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="C4" pad="1"/>
<contactref element="U2" pad="24"/>
</signal>
<signal name="TEST">
<contactref element="U2" pad="17"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="5"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="2"/>
<contactref element="XTAL" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U2" pad="1"/>
<contactref element="XTAL" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
